BRIZA SINGLE

Playful, yet moderate. Eccentric, yet balanced. Anytime,

Product: Briza Single, vertical round tube on tube design radiator

Also supplied: 4 white brackets (in chrome for any other radiator colour), screws, plugs, anti-lift clip,

bracket hiders, design air vent and design blind plug, blind plugs and assembly instructions

Connections: 4 x ½” female connection (centre connection included)

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: height – length.

Warranty: 10 years, as long as the installation instructions have been followed, Stelrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated, primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 6 bar (tested at 7,8 bar) Max. operating temperature: 95 °C

Conformity: in accordance with EN442

Heights: 1.800 | 2.000 mm

Number of tubes: 12 | 14 | 16 | 18

Lengths: 447 | 521 | 595 | 669 mm

Tubes : vertical, O-section, diameter 22 mm

Collector: horizontal, O-section, diameter 38 mm