COMPACT STYLE

The decorative Compact Style radiator features horizontal lines creating an atmosphere of space and sophistication. A compact radiator that has a stylish front panel, with close-fitting side panels and decorative upper grille giving your home a neat and distinctive appearance.

Product: decorative encased panel radiator with a stylish front plate

Finishing: decorative stylish front with upper grille and side panels

Also supplied: VDI brackets (type Monclac), screws, plugs, air vent, blind plug and installation instructions

Connections: 4 x ½” female connection

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 21 | 22 | 33

Heights: 300 | 400 | 500 | 600 | 700 | 900 mm

Lengths: 400 – 2.000 mm

Depths: 79 | 102 | 160 mm