DAHLIA | DAHLIA CT

The Dahlia is a traditional bathroom radiator that retains the timeless character of the bathroom with its simplicity and symmetry of straight, round tubes and D-shaped collectors. This radiator can also be used as a partition wall to create separate areas. Also available with a centre connection.

Product: the classic bathroom radiator, also available with a centre connection

Also supplied: wall brackets, screws, plugs, air vent and blind plugs

Connections: 4 x ½” female connection (6 x ½” if with centre connection)

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 5 years, as long as the installation instructions have been followed, Stelrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 95 °C

Conformity: in accordance with EN442

Heights: 775 | 1.181 | 1.411 | 1.763 | 1.993 mm

Number of tubes: 16 | 24 | 28 | 36 | 40

Lengths: 495 | 585 | 737 mm

Tubes: horizontal, O-section, diameter 22 mm

Collector: vertical, D-section