HORTA DOUBLE

Extra comfort, extra design.

Product: Verona Double, vertical flat tube on tube design radiator

Also supplied: 4 brackets (in radiator colour), screws, plugs, anti-lift clip, design air vent and design blind plug, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: height – length.

Warranty: 10 years, as long as the installation instructions have been followed, Stelrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated, primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 4 bar (tested at 5,2 bar) Max. operating temperature: 95 °C

Conformity: in accordance with EN442

Heights: 1.600 | 1.800 | 2.000 mm

Number of tubes: 20 | 24 | 28 | 32 | 36

Lengths: 488 | 588 | 688 | 788 | 888 mm Tubes : vertical, 60 x 10 mm flat section Collector: horizontal, O-section, diameter 38 mm