HYGIENE

The Hygiene radiator is a panel radiator without convection fins, upper grille or side panels, made from

high-quality steel. A classic icon.

Product: a classic panel radiator without convection fins Finishing: without convection fins, upper grille or side panels Connections: 4 x ½” female connection

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Heat cost allocator: Suitable for heat cost allocators, both electronic and according to the evaporation principle

(covered by the norm of EN834 & EN835).

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: RAL and NF

Types: 10 | 20 | 30

Heights: 300 | 400 | 500 | 600 | 700 | 900 mm

Lengths: 400 – 3.000 mm

Depths: 47 | 77 | 158 mm