NOVELLO PLINTH

The Novello Plinth offers the perfect solution for spaces with large window sections from floor to ceiling, like shop windows, verandas and winter gardens. Its subtle construction means this radiator perfectly matches any interior. The cold air close to a window is heated to provide warmth. The Novello Plinth can be connected either as a valve or compact radiator.

Product: fully encased valve radiator with a height of 200 mm

Finishing: upper grille and side panels

Pre-installed: adjustable Heimeier valve type insert 4368

Valve insert: The integrated adjustable valve insert (without thermostatic head) is factory-fit on the right side of the radiator, CEN certified, tested in accordance with EN215 and compatible with thermostatic heads M30 x 1,5mm.

Also supplied: air vent and blind plugs

Connections: 6 x ½” female connection (2 x ½” lateral bottom connection included) Lugs: no lugs

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty

conditions have been met.

Paint process: All radiators are degreased, phosphated, primed and powder-coated in Stelrad white 9016 as

standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Heat cost allocator: Suitable for heat cost allocators, both electronic and according to the evaporation principle

(covered by the norm of EN834 & EN835).

Max. operating pressure: 10 bar (tested at 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 22 | 33 | 44

Height: 200 mm

Lengths: 1.000 – 2.600 mm

Depths: 100 | 158 | 216 mm