PLANAR ECO

The Planar ECO radiator unites design with our serial flow technology (water flows first through the front panel) and is perfectly suited for heating systems that work with low operating temperatures. This ECO technology results in high energy efficiency, maximum radiation, faster heating rate and less waste of energy. The combination of this technology with the flat front, a design upper grille and side panels allows you to enjoy our green heat technology in style and luxury.

Product: decorative Stelrad ECO valve radiator ideally suited for low-temperatures heating system and equipped with our serial flow technology, both a centre and lateral bottom connection, a pre-set valve insert (which can be fitted on the left or right side of the radiator) and with a decorative flat front

Finishing: decorative flat front, upper grille and side panels

Pre-installed: pre-set Heimeier 4368 or 4369 valve insert, ECO air vent and blind plugs

Valve insert: The integrated adjustable valve insert (without thermostatic head) is factory-fit on the right side of the radiator, CEN certified, tested in accordance with EN215 and compatible with thermostatic heads M30 x 1,5 mm. The valve insert can also be fitted on the left side of the radiator.

The thermostatic valve insert is factory-set in relation to the size of the radiator. This pre-setting ensures optimum throughput in the radiator. Factory setting for two-pipe systems, also suitable for one-pipe systems (as long as the valve insert is adjusted to position 8).

Also supplied: VDI brackets (type Monclac), screws, plugs and assembly instructions

Connections: 2 x ¾” male eurocone centre connection and 2 x ½” female lateral bottom connection

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 21 | 22 | 33

Heights: 300 | 400 | 500 | 600 | 700 | 900 mm

Lengths: 400 – 2.000 mm

Depths: 79 | 102 | 160 mm