PLANAR SLIM ECO

The age of radiators being hidden came to a definite end with the arrival of the Planar Slim ECO.

You’ll actually want to highlight this radiator. The bi-colour design with a completely smooth front and recessed black upper grille and side panels gives the radiator an unrivalled look. Its high-quality finish offers you an attractive and warm radiator for years on end. Use it in combination with the Vertex Slim to create a light and spacious feel throughout your home.

Product: decorative horizontal low-temperature valve radiator with serial flow technology, both a centre and lateral bottom connection and a pre-set valve insert, which can be fitted on the left or right side of the radiator

Finishing: completely smooth design with a jointless front and recessed black upper grille and side panels

Pre-installed: pre-set Heimeier 4368 valve insert, ECO air vent and blind plugs

Valve insert: The integrated adjustable valve insert is factory-fit on the right side of the radiator, CEN

certified, tested in accordance with EN215 and compatible with thermostatic heads M30 x

1,5mm. The valve insert can also be fitted on the left of the ECO radiator.

The thermostatic valve insert is factory-set in relation to the size of the radiator. This pre- setting ensures optimum throughput in the radiator. Factory setting for two-pipe systems, also suitable for one-pipe systems (as long as the valve insert is adjusted to position 8).

Also supplied: design thermostatic head, valve insert spindle extension, wall brackets, screws, plugs and assembly instructions

Connections: 2 x ¾” male Eurocone centre connection and 2 x ½” female lateral bottom connection

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged with protective foam-filled bags, in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in

Stelrad SN170 black as standard.

Colours front panel: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Colour side panels and upper grille: SN170 black

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 21 | 22

Heights: 545 | 645 mm

Lengths: 1.070 | 1.270 | 1.470 | 1.670 | 1.870 | 2.070 mm

Depths: 96 | 119 mm