PLANAR STYLE

With the interplay of horizontal contours in combination with a complimentary colour, the decorative Planar Style provides an atmosphere of peace and serenity. The Planar Style can be connected either as a valve or compact radiator and forms an attractive combination with the vertical Vertex Style models and Compact Line for harmonious unity in the home.

Product: decorative valve radiator with a stylish front

Finishing: decorative stylish front, upper grille and side panels

Pre-installed: pre-set Heimeier 4368 or 4369 valve insert, air vent and blind plugs

Valve insert: The integrated adjustable valve insert (without thermostatic head) is factory-fit on the right side of the radiator, CEN certified, tested in accordance with EN215 and compatible with thermostatic heads M30 x 1,5mm.

The thermostatic valve insert is factory-set in relation to the size of the radiator. This pre-setting ensures optimum throughput in the radiator. Factory setting for two-pipe systems, also suitable for one-pipe systems (as long as the valve insert is adjusted to position 8).

Also supplied: VDI brackets (type Monclac), screws, plugs and installation instructions

Connections: 6 x ½” female connection (2 x ½” lateral bottom connection included). Left version is available

on request.

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty

conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad

white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: RAL and NF Types: 11 | 21 | 22 | 33

Heights: 300 | 400 | 500 | 600 | 700 | 900 mm

Lengths: 500 – 2.000 mm

Depths: 63 | 79 | 102 | 160 mm