PLANAR STYLE PLINTH D

Low radiators are highly suitable for spaces with large floor-to-ceiling windows. The cold air from a window is immediately converted into pleasant warmth. With a stylised front and rear, a decorative upper grille and side panels the Planar Style Plinth D radiator ensures optimal warmth with a minimum of height and a great double finish! Moreover this radiator can be connected either as a valve or as a compact radiator.

Product: decorative valve radiator with a stylish front and rear and a height of 200 mm

Finishing: decorative stylish front and rear, upper grille and side panels

Pre-installed: adjustable Heimeier valve insert type 4368

Valve insert: The integrated adjustable valve insert (without thermostatic head) is factory-fit on the right side of the radiator, CEN certified, tested in accordance with EN215 and compatible with thermostatic heads M30 x 1,5mm.

Also supplied: air vent and blind plugs

Connections: 6 x ½” female connection (2 x ½” lateral bottom connection included).

Lugs: no lugs

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 22 | 33 | 44

Height: 200 mm

Lengths: 1.000 – 2.600 mm

Depths: 104 | 162 | 220 mm