PLANAR STYLE PLINTH

Are you having problems finding a suitable radiator for your large window sections? The Planar Style Plinth offers you the perfect solution. This plinth radiator is equipped with one stylised fronts, a decorative upper grille and side panels. In combination with the Compact Style, Planar Style or Vertex Style its horizontal play of lines ensures design consistency throughout your home. The radiator can be connected either as a valve or as a compact radiator.

Product: decorative valve radiator with a stylish front and a height of 200 mm

Finishing: decorative stylish front, upper grille and side panels

Pre-installed: adjustable Heimeier valve insert type 4368

Valve insert: The integrated adjustable valve insert (without thermostatic head) is factory-fit on the right side of the radiator, CEN certified, tested in accordance with EN215 and compatible with thermostatic heads M30 x 1,5mm.

Also supplied: air vent and blind plugs

Connections: 6 x ½” female connection (2 x ½” lateral bottom connection included). Lugs: no lugs

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 22 | 33 | 44

Height: 200 mm

Lengths: 1.000 – 2.600 mm

Depths: 102 | 160 | 218 mm