RENO COMPACT

A Compact radiator with a very specific centre distance to replace old cast-iron and ribbed radiators while using the existing piping system.

Product: the fully encased compact radiator specifically developed for the renovation market

Finishing: upper grille and side panels Also supplied: assembly instructions Connections: 4 x ½” female connection

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Heat cost allocator: Suitable for heat cost allocators, both electronic and according to the evaporation principle

(covered by the norm of EN834 & EN835). Max. operating pressure: 10 bar (tested at 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: RAL

Types: 21 | 22 | 33

Heights: 400 | 550 | 950 mm Lengths: 400 – 3.000 mm Depths: 77 | 100 | 158 mm