VERTEX PLAN

The Vertex Plan combines a sleek and decorative appearance and is perfect for applications where wall space is at a premium. This radiator can be perfectly combined with the Planar to provide a modern design and consistent look throughout your whole home.

Product: decorative vertical radiator with a centre connection and a flat front

Finishing: decorative flat front and side panels

Also supplied: wall brackets, ETA safety screws and plugs, screws and plugs, air vent, blind plugs and assembly instructions

Connections: 4 x ½” female connection (centre connection included) Lugs: no lugs

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

 The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: RAL and NF Types: 11 | 20 | 21 | 22

Heights: 1.600 | 1.800 | 2.000 | 2.200 mm Lengths: 300 | 400 | 500 | 600 | 700 mm Depths: 49 | 79 | 79 | 102 mm