VERTEX SLIM

The Vertex Slim is the ultimate design radiator for anyone preferring a sleek and masterly design. The completely uniform front and recessed black side panels and upper grille give the radiator an unparalleled aura. Its excellent bi-colour finish adds extra class to your home, even if the space is limited.

Product: decorative vertical radiator with a centre connection and a smooth front panel and flush black

side panels

Finishing: completely smooth design with jointless recessed black side panels

Also supplied: wall brackets, ETA safety screws and plugs, screws and plugs, air vent, blind plugs and

assembly instructions

Connections: 4 x ½” female connection (centre connection included) Lugs: no lugs

Packaging: Every radiator is sturdily packaged with protective foam-filled bags, in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty

conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad

white 9016 as standard.

Colours front panel: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Colour side panel: SN170 black

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 11 | 21 | 22

Heights: 1.840 | 2.040 mm Lengths: 470 | 570 | 670 mm Depths: 73 | 96 | 119 mm