VERTEX STYLE

In both traditional and trendy newly build and renovation projects large glazed sections and terrace windows are often used to optimise natural lighting and thus limiting the open wall space. With the Vertex Style Stelrad offers you the ideal solution. When combining the Vertex Style with Planar Style and Compact Style models a light and spacious feeling is created throughout your home.

Product: decorative vertical radiator with a centre connection and a stylised front

Finishing: decorative stylised front and side panels

Also supplied: wall brackets, ETA safety screws and plugs, screws and plugs, air vent, blind plugs and assembly instructions

Connections: 4 x ½” female connection (centre connection included) Lugs: no lugs

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic.

The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar) Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: RAL

Types: 11 | 20 | 21 | 22

Heights: 1.600 | 1.800 | 2.000 | 2.200 mm Lengths: 300 | 400 | 500 | 600 | 700 mm Depths: 49 | 79 | 79 | 102 mm