VERTEX TANGO

With its natural sleek contours the Vertex Tango creates allure in any interior. Whether you choose a minimalist look or a cosy warm atmosphere, its seamless angular finish makes the Vertex Tango stylish and uniform in every way. Choose one of our colours to find the perfect harmony between your home and your Vertex Tango radiator.

Product: decorative vertical radiator with a centre connection, a minimum distance to the wall and a neat angular look

Finishing: completely smooth, angled design

Also supplied: wall brackets, ETA safety screws and plugs, screws and plugs, air vent, blind plugs and assembly instructions

Connections: 4 x ½” female connection (centre connection included) Lugs: no lugs

Packaging: Every radiator is sturdily packaged with protective foam-filled bags, in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad

white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested at 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 11 | 21 | 22

Heights: 1.820 | 2.020 mm Lengths: 410 | 510 | 610 mm Depths: 73 | 96 | 119 mm