VALERIANA - VALERIANA CT

A bathroom is often also a place for slowing down, beauty and relaxation. The Valeriana bathroom radiator enhances this feeling of wellbeing in its own way with its aesthetic design.

This Stelrad Valeriana radiator with its curved and round tubes emphasises elegance, and with its discreet presence ensures your heating comfort. Also available with a centre connection.

Product: elegant bathroom radiator, also available with a centre connection

Also supplied: wall brackets, screws, plugs, air vent blind plugs and installation instructions

Connections: 4 x ½” female connection (6 x ½” if with centre connection)

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed, Stelrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 95 °C

Conformity: in accordance with EN442

Heights: 775 | 1.181 | 1.763 mm

Number of tubes: 16 | 24 | 36

Lengths: 495 | 585 | 737 mm

Tubes: horizontal, curved, O-section, diameter 22 mm

Collector: vertical, D-section