CLOUD

The Cloud is a smooth fronted, curved faced steel radiator. Using dry inertia technology, the radiator heats the air in your rooms via a process of convection, offering exceptional warmth and remarkable energy efficiency wrapped up in a single solution.

Product: Electric dry inertia radiator

Pre-installed: Thermostat and a 1,2 m insulated cable with plug.

Also supplied: Brackets, screws, plugs and manual

Control: Control via an integrated thermostat with automatic weekly programming, open window detection, presence detection and boost function.

Packaging: Every radiator is sturdily packaged in high-quality cardboard. The radiator’s characteristics are shown on the label: electric power – height – length.

Warranty: 10 years for the radiator and 2 years for the electrical components, as long as the installation instructions have been followed, Stelrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated and powder-coated.

Colours: Traffic white or anthracite grey

Conformity: EcoDesign 2018 (EU Regulation 2015/1188)

Technical data: Voltage 230V ~50Hz, IP24, Class II

Height: 600 mm

Lengths: 470 | 550 | 830 | 1.040 mm

Depth: 83 mm

Output: 700 | 1.000 | 1.500 | 2.000 W