DAHLIA E

With the electrical version of the Dahlia radiator a new era is upon us. Nowadays alternative energy sources also get more interest next to the traditional hydraulic heating. The Dahlia E is Stelrad’s answer to this evolution.

Product: Electrical classic bathroom radiator

Pre-installed: Prefilled with heating liquid and including mounted thermostat.
Available as a version with 0,8 m insulated cable without plug and as a version with 1,2 m insulated cable with plug.

Also supplied: Brackets, screws, plugs and manual

Control: Operated via integrated thermostat with weekly programming, open window detection and boost function. IR receiver for the optional remote control.

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years for the radiator and 2 years for the electrical components, as long as the installation instructions have been followed, Stelrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated, primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Conformity: EcoDesign 2018 (EU Regulation 2015/1188)

Technical data: Voltage 230V ~50Hz, IP44, Class II

Heights: 775 | 1.181 | 1.411 | 1.763 mm

Number of tubes: 16 | 24 | 28 | 36

Lengths: 400 | 450 | 495 | 585 mm

Output: 400 | 500 | 600 | 700 | 900 | 1.000 W

Tubes: horizontal, O-section, diameter of 22 mm