GILIA DOUBLE

The double version for unmatched comfort.

Product: Gilia Double, vertical round tube-on-tube design radiator

Also supplied: 4 white brackets (in chrome for any other radiator colour), screws, plugs, design air vent and design blind plug, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: height – length.

Warranty: 10 years, as long as the installation instructions have been followed, Stelrad’s warranty conditions have been met and the radiator is installed outside the splash area.

Paint process: All radiators are degreased, phosphated and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 6 bar (tested to 7,8 bar)

Max. operating temperature: 95 °C

Conformity: in accordance with EN442

Heights: 1.199 | 1.495 | 1.791 | 2.013 mm

Number of tubes: 56 | 68 | 84 | 96

Lengths: 500 | 600 | 750 | 900 mm

Tubes: horizontal, O-section, diameter of 22 mm

Collector: vertical, O-section, diameter 38 mm