NOVELLO MATERNELLE

The Novello Maternelle is an encased valve radiator with a non-water-supplied front plate. It is specially designed for nurseries, kindergartens and retirement homes. The contact surface of the front plate remains at a low temperature at all times, ensuring the safety of everyone from children to adults.

Product: the fully encased valve radiator with a non-water-supplied front plate

Finishing: upper grille and side panels

Pre-installed: preset Heimeier 4368 or 4369 valve insert, air vent and blind plugs

Valve insert: The integrated adjustable valve insert (without thermostatic head) is factory-fit on the right side of the radiator, CEN certified, tested in accordance with EN215 and compatible with thermostatic heads M30 x 1,5 mm.

The thermostatic valve insert is factory-set in relation to the size of the radiator. This presetting ensures optimum throughput in the radiator. Factory setting for two-pipe systems, also suitable for one-pipe systems (as long as the valve insert is adjusted to position 8).

Also supplied: VDI brackets (Type Monclac), screws, plugs and installation instructions

Connections: 6 x ½” female connection (Left handed version is available on request)

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: NF

Type: 32

Heights: 400 | 600 | 700 mm

Lengths: 400 – 2.400 mm

Depths: 158 mm