VERTEX

Do you only have limited space to fit a radiator? The Vertex is the solution. This vertical radiator takes up a minimum of space and optimally heats the cold air next to large window section.

Product: vertical panel radiator with a centre connection

Finishing: side panels (only for types 11, 20, 21 and 22)

Also supplied: wall brackets, ETA safety screws and plugs, screws, plugs, air vent, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included). Types 20, 21 and 22 can be reversed (front/back), in which case inlet and outlet are also reversed.

Lugs: no lugs

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Heat cost allocator: Suitable for heat cost allocators, both electronic and according to the evaporation principle (covered by the norm of EN834 & EN835).

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Quality assurance: NF

Types: 10 | 11 | 20 | 21 | 22

Heights: 1.600 | 1.800 | 2.000 | 2.200 mm

Lengths: 300 | 400 | 500 | 600 | 700 mm

Depths: 47 | 47 | 77 | 77 | 100 mm