VERTEX SWING

With its attractive round contours the Vertex Swing radiator is set to charm anyone. Its specific design not only makes it look graceful, it also provides heating performance that exceeds expectations. You can also have the colour of the Vertex Swing seamlessly merge into your interior, or use it as an eye-catcher to give the space extra character. Whatever choices you make, the Vertex Swing offers you the ultimate solution.

Product: decorative vertical radiator with a centre connection, a minimum distance to the wall and round curves

Finishing: completely smooth, rounded design

Also supplied: wall brackets, ETA safety screws and plugs, screws, plugs, air vent, blind plugs and installation instructions

Connections: 4 x ½” female connection (centre connection included)

Lugs: no lugs

Packaging: Every radiator is sturdily packaged with protective foam-filled bags, in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 21 | 22

Heights: 1.820 | 2.020 mm

Lengths: Type 21: 504 | 604 | 704 mm  
 Type 22: 527 | 627 | 727 mm

Depths: 96 | 119 mm