RENO PLANAR

The Reno Planar is a compact radiator, with a beautiful decorative flat front, specially designed for use in home renovations. Its very specific dimensions make it possible to replace the old cast iron and column radiators while preserving the existing pipes. Simple and quick installation is possible without conversion. In addition, this radiator offers the same advantages as a compact radiator thanks to its finish with a sturdy housing and decorative grille.

Product: the fully encased compact radiator with a flat front specifically developed for the renovation market

Finishing: decorative flat front, upper grille and side panels

Also supplied: installation instructions

Connections: 4 x ½” female connection

Lugs: 2 pairs of mounting lugs up to 1.600 mm and 3 pairs from 1.800 mm

Packaging: Every radiator is sturdily packaged in high-quality cardboard and wrapped in plastic. The radiator’s characteristics are shown on the label: type – height – length.

Warranty: 10 years, as long as the installation instructions have been followed and Stelrad’s warranty conditions have been met.

Paint process: All radiators are degreased, phosphated, cataphoretically primed and powder-coated in Stelrad white 9016 as standard.

Colours: Stelrad white 9016 + 35 different Stelrad colours and about 200 RAL-colours are possible

Max. operating pressure: 10 bar (tested to 13 bar)

Max. operating temperature: 110 °C

Conformity: in accordance with EN442

Types: 21 | 22 | 33

Heights: 550 | 950 mm

Lengths: 400 – 2.000 mm

Depths: 79 | 102 | 160 mm